Cleaning Hardwood Floors

Cleaning a hardwood floor is not the same as it was 30 years ago. Gone are the days of sore knees and aching backs from waxing wood floors. In fact, waxing or polishing floors is a mistake and will damage them for the long term. NEVER WAX A WOOD FLOOR unless it is recommended by the manufacturer, as today’s urethane floor finishes are very good and will hold up well with a little maintenance.

Grit and water are your floors biggest enemies. Grit acts like sandpaper under your feet and furniture. While puddled water will cup or even blacken your floor if left without clean up. Water and pet urine must be cleaned up immediately and kept from soaking into carpets and area rugs to avoid permanent damage. 

That brings us to the most common question we are asked, “How do I clean and maintain my hardwood floors?”

For best results follow these guidelines:

•	You may vacuum your floors as often as you like. A central vacuum system is excellent, as there are no wheels to pull around; however, a household vacuum will work very well with a soft bristle.
•	Dust mop your floor often, as this is easy on the floor and will remove grit.
•	Damp mop your floor only when needed to clean spills. For regular maintenance, Squeaky Clean, made by Basic Coatings, is one of the many excellent floor-cleaning products available. Do not wet mop.
•	Do not use any products containing ammonia.
•	When areas begin to show wear, consult a flooring finisher. If you have not used a wax base cleaner, polish or dusting spray, you will be able to have your floor screen sanded, followed by one or two coats of urethane finish. Your floor again will have its luster and durability. This preventative maintenance should be considered between the 5-10 year mark depending on wear.
•	Place protective pads under all chairs and movable furniture that is in direct contact with the floor. Most hardware, department and flooring stores carry protective pads. 
•	Place throw rugs is high traffic areas, such as entrance doors and hallways.
•	High heels will stress a floor. A 125 lb. person will exert 2000 pounds of pressure on the floor.
•	Check water lines of dishwashers, ice makers, sinks and washing machines regularly to avoid damages caused by unseen leaks.

Follow the recommendations of your flooring manufacturer, as there are many types of flooring on the market today. Disregarding their recommendations may nullify any guarantee. 

Unlike most floor coverings, hardwood floors are a long-term investment when correctly maintained, will add beauty and value for the lifetime of the home.

Heister House Millworks, Inc.
1937 Troup Valley Road  * Mt. Pleasant Mills, PA  17853-9761
Phone: 570-539-2611 * 800-326-9873 * Fax: 570-539-2379 * 800-718-4463
hhmillworks.com